**LEGENDS**

Figure 1 – Representative image in lateral aspect of the light booth, with device positioned for sample disposition.

Figure 2 – Percentage of surface gloss perceptibility according to the different tested illuminants: D65, Incandescent, and Fluorescent lights, under different ∆GU comparisons.

Figure 3 – Percentage of gloss perceptibility for all observers regarding ∆GU intervals.

Figure 4 – Non-linear estimate curve and the resulted limit of gloss perceptibility (17.6 ∆GU).